**Test input file for ABAQUS 6.6-4, D. Masin, masin@natur.cuni.cz
*HEADING
Drained triaxial test, soft Cam clay model
*NODE,NSET=ALLN
*ELEMENT,TYPE=CAX4,ELSET=ALLE
*SOLID SECTION,ELSET=ALLE,MATERIAL=USERMAT
*MATERIAL,NAME=USERMAT
*DEPVAR
*USER MATERIAL, CONSTANTS=10, UNSYMM
*BOUNDARY
 1,PINNED
 2,2
 4,1
*INITIAL CONDITIONS, TYPE=SOLUTION, USER
*INITIAL CONDITIONS,TYPE=STRESS
 ALLE,-100.,-100.,-100.,0.
*STEP,INC=1
*STATIC
1
*DLOAD
 102,P2,100.
 102,P3,100.
*EL PRINT, ELSET=ALLE
S, E
*NODE PRINT
 U,
 RF,
*EL FILE,FREQ=10
 S,E,PE
*END STEP
*STEP,INC=10000
*STATIC
1.d-3, 1., 1.d-4, 1.d-2
*BOUNDARY
 3,2,,-.4
 4,2,,-.4
*END STEP